University of Texas at El Paso
Radiation Survey

Building				Room #		Department				

Authorized User						Survey for Month			

Radionuclides in use:  32P  33P  35S  3H  14C  125I     Others						

	




















Counting equipment:						Calibration Date:				

Calibration radioisotope:					Counter type:   gamma   LSC   other

Energy range:				Bkgrd count:		cpm		Efficiency			

Wipe Results

Isotope

DPM

DPM=(cpm-bkgrd)/efficiency

If excessive contamination is found, describe on the back of this form the corrective actions taken.  Include all dates and results of resultant wipe tests.


Name:								Survey Date:					
